Residential Pickets and Picket Fence Quote Request Form

Please complete the below form for all loose pickets and picket fencing enquires and email to sales@replas.com.au

A sales team member will be in touch and supply a quote within 3 working days.

|  |  |
| --- | --- |
| Customer nameEmail and contact details.Please include State |  |
|  |
| Project name, location and timeframe |  |
| Delivery Location:Availability of a forklift for unloading. |  |
| Total lineal metres of project including all gates |  |
| Number of pedestrian access gates | 900mm width | QTY: |
| Number and width of vehicle access gatesmaintenance gates | Width: | QTY: |
| Width: | QTY: |
| Size of Pickets Standard 800mm (900mm high fence) 900mm or 1200mm available (non-standard sizes can be supplied subject to MOQ) | Picket Height:  |
| Picket Thickness – 12mm or 18mmPicket Width (standard width is 62mm): |
| Gap between the pickets | Either 20mm or 45mm: |
| Style of Pickets, Please nominate: |  |
| Colour of picketsPlease nominate:Colour of posts, gate frames and railsPlease nominate: | Standard colours are:Off White (= Colorbond Surfmist ®)Smooth Cream (= Colorbond Classic Cream ®)Mist Green (= Colorbond Pale Eucalypt ®)Caulfield Green (= Colorbond Cottage Green ®)Slate Grey (= Colorbond Woodland Grey ®)Charcoal (= Colorbond Night Sky ®)(Other colours can be supplied subject to MOQ) |