Residential Pickets and Picket Fence Quote Request Form

Please complete the below form for all loose pickets and picket fencing enquires and email to [sales@replas.com.au](mailto:sales@replas.com.au)

A sales team member will be in touch and supply a quote within 3 working days.

|  |  |  |
| --- | --- | --- |
| Customer name  Email and contact details.  Please include State |  | |
|  | |
| Project name, location and timeframe |  | |
| Delivery Location:  Availability of a forklift for unloading. |  | |
| Total lineal metres of project including all gates |  | |
| Number of pedestrian access gates | 900mm width | QTY: |
| Number and width of  vehicle access gates  maintenance gates | Width: | QTY: |
| Width: | QTY: |
| Size of Pickets  Standard 800mm (900mm high fence) 900mm or 1200mm available  (non-standard sizes can be supplied subject to MOQ) | Picket Height: | |
| Picket Thickness – 12mm or 18mm  Picket Width (standard width is 62mm): | |
| Gap between the pickets | Either 20mm or 45mm: | |
| Style of Pickets,  Please nominate: |  | |
| Colour of pickets  Please nominate:  Colour of posts, gate frames and rails  Please nominate: | Standard colours are:  Off White (= Colorbond Surfmist ®)  Smooth Cream (= Colorbond Classic Cream ®)  Mist Green (= Colorbond Pale Eucalypt ®)  Caulfield Green (= Colorbond Cottage Green ®)  Slate Grey (= Colorbond Woodland Grey ®)  Charcoal (= Colorbond Night Sky ®)  (Other colours can be supplied subject to MOQ) | |